



@deftypefun {int} {gnutls_x509_crl_list_import} (gnutls_x509_crl_t * @var{crls}, unsigned int * @var{crl_max}, const gnutls_datum_t * @var{data}, gnutls_x509_crt_fmt_t @var{format}, unsigned int @var{flags})
@var{crls}: Indicates where the parsed CRLs will be copied to. Must not be initialized.

@var{crl_max}: Initially must hold the maximum number of crls. It will be updated with the number of crls available.

@var{data}: The PEM encoded CRLs

@var{format}: One of DER or PEM.

@var{flags}: must be (0) or an OR'd sequence of gnutls_certificate_import_flags.

This function will convert the given PEM encoded CRL list
to the native gnutls_x509_crl_t format. The output will be stored
in  @code{crls} .  They will be automatically initialized.

If the Certificate is PEM encoded it should have a header of "X509 CRL".

@strong{Returns:} the number of certificates read or a negative error value.

@strong{Since:} 3.0
@end deftypefun
