



@deftypefun {int} {gnutls_x509_crt_list_import2} (gnutls_x509_crt_t ** @var{certs}, unsigned int * @var{size}, const gnutls_datum_t * @var{data}, gnutls_x509_crt_fmt_t @var{format}, unsigned int @var{flags})
@var{certs}: Will hold the parsed certificate list.

@var{size}: It will contain the size of the list.

@var{data}: The PEM encoded certificate.

@var{format}: One of DER or PEM.

@var{flags}: must be (0) or an OR'd sequence of gnutls_certificate_import_flags.

This function will convert the given PEM encoded certificate list
to the native gnutls_x509_crt_t format. The output will be stored
in  @code{certs} which will allocated and initialized.

If the Certificate is PEM encoded it should have a header of "X509
CERTIFICATE", or "CERTIFICATE".

To deinitialize  @code{certs} , you need to deinitialize each crt structure
independently, and use @code{gnutls_free()}  at

@strong{Returns:} the number of certificates read or a negative error value.

@strong{Since:} 3.0
@end deftypefun
