- NAME
- SYNOPSIS
- DESCRIPTION
- GENERATION STRING FORMAT

- SUPPORTED TYPES
- MODIFIERS

- EXAMPLES
- RETURN VALUES
- SEE ALSO
- HISTORY

# NAME

ASN1_generate_nconf, ASN1_generate_v3 - ASN1 generation functions

# SYNOPSIS

     #include <openssl/asn1.h>

     ASN1_TYPE *ASN1_generate_nconf(char *str, CONF *nconf);
     ASN1_TYPE *ASN1_generate_v3(char *str, X509V3_CTX *cnf);

# DESCRIPTION

These functions generate the ASN1 encoding of a string in an ASN1_TYPE structure.

str contains the string to encode nconf or cnf contains the optional configuration information where additional strings will be read from. nconf will typically come from a config file wherease cnf is obtained from an X509V3_CTX structure which will typically be used by X509 v3 certificate extension functions. cnf or nconf can be set to NULL if no additional configuration will be used.

# GENERATION STRING FORMAT

The actual data encoded is determined by the string str and the configuration information. The general format of the string is:

[modifier,]type[:value]

That is zero or more comma separated modifiers followed by a type followed by an optional colon and a value. The formats of type, value and modifier are explained below.

## SUPPORTED TYPES

The supported types are listed below. Unless otherwise specified only the ASCII format is permissible.

BOOLEAN, BOOL

  This encodes a boolean type. The value string is mandatory and should be TRUE or FALSE. Additionally TRUE, true, Y, y, YES, yes, FALSE, false, N, n, NO and no are acceptable.

NULL

  Encode the NULL type, the value string must not be present.

INTEGER, INT

  Encodes an ASN1 INTEGER type. The value string represents the value of the integer, it can be preceeded by a minus sign and is normally interpreted as a decimal value unless the prefix 0x is included.

ENUMERATED, ENUM

  Encodes the ASN1 ENUMERATED type, it is otherwise identical to INTEGER.

OBJECT, OID

  Encodes an ASN1 OBJECT IDENTIFIER, the value string can be a short name, a long name or numerical format.

UTCTIME, UTC

  Encodes an ASN1 UTCTime structure, the value should be in the format YYMMDDHHMMSSZ.

GENERALIZEDTIME, GENTIME

  Encodes an ASN1 GeneralizedTime structure, the value should be in the format YYYYMMDDHHMMSSZ.

OCTETSTRING, OCT

  Encodes an ASN1 OCTET STRING. value represents the contents of this structure, the format strings ASCII and HEX can be used to specify the format of value.

BITSTRING, BITSTR

  Encodes an ASN1 BIT STRING. value represents the contents of this structure, the format strings ASCII, HEX and BITLIST can be used to specify the format of value.

  If the format is anything other than BITLIST the number of unused bits is set to zero.

UNIVERSALSTRING, UNIV, IA5, IA5STRING, UTF8, UTF8String, BMP, BMPSTRING, VISIBLESTRING, VISIBLE, PRINTABLESTRING, PRINTABLE, T61, T61STRING, TELETEXSTRING, GeneralString, NUMERICSTRING, NUMERIC

  These encode the corresponding string types. value represents the contents of this structure. The format can be ASCII or UTF8.

SEQUENCE, SEQ, SET

  Formats the result as an ASN1 SEQUENCE or SET type. value should be a section name which will contain the contents. The field names in the section are ignored and the values are in the generated string format. If value is absent then an empty SEQUENCE will be encoded.

## MODIFIERS

Modifiers affect the following structure, they can be used to add EXPLICIT or IMPLICIT tagging, add wrappers or to change the string format of the final type and value. The supported formats are documented below.

EXPLICIT, EXP

  Add an explicit tag to the following structure. This string should be followed by a colon and the tag value to use as a decimal value.

  By following the number with U, A, P or C UNIVERSAL, APPLICATION, PRIVATE or CONTEXT SPECIFIC tagging can be used, the default is CONTEXT SPECIFIC.

IMPLICIT, IMP

  This is the same as EXPLICIT except IMPLICIT tagging is used instead.

OCTWRAP, SEQWRAP, SETWRAP, BITWRAP

  The following structure is surrounded by an OCTET STRING, a SEQUENCE, a SET or a BIT STRING respectively. For a BIT STRING the number of unused bits is set to zero.

FORMAT

  This specifies the format of the ultimate value. It should be followed by a colon and one of the strings ASCII, UTF8, HEX or BITLIST.

  If no format specifier is included then ASCII is used. If UTF8 is specified then the value string must be a valid UTF8 string. For HEX the output must be a set of hex digits. BITLIST (which is only valid for a BIT STRING) is a comma separated list of the indices of the set bits, all other bits are zero.

# EXAMPLES

A simple IA5String:

     IA5STRING:Hello World

An IA5String explicitly tagged:

     EXPLICIT:0,IA5STRING:Hello World

An IA5String explicitly tagged using APPLICATION tagging:

     EXPLICIT:0A,IA5STRING:Hello World

A BITSTRING with bits 1 and 5 set and all others zero:

     FORMAT:BITLIST,BITSTRING:1,5

A more complex example using a config file to produce a SEQUENCE consiting of a BOOL an OID and a UTF8String:

     asn1 = SEQUENCE:seq_section

     [seq_section]

     field1 = BOOLEAN:TRUE
     field2 = OID:commonName
     field3 = UTF8:Third field

This example produces an RSAPrivateKey structure, this is the key contained in the file client.pem in all OpenSSL distributions (note: the field names such as 'coeff' are ignored and are present just for clarity):

     asn1=SEQUENCE:private_key
     [private_key]
     version=INTEGER:0

     n=INTEGER:0xBB6FE79432CC6EA2D8F970675A5A87BFBE1AFF0BE63E879F2AFFB93644\
     D4D2C6D000430DEC66ABF47829E74B8C5108623A1C0EE8BE217B3AD8D36D5EB4FCA1D9

     e=INTEGER:0x010001

     d=INTEGER:0x6F05EAD2F27FFAEC84BEC360C4B928FD5F3A9865D0FCAAD291E2A52F4A\
     F810DC6373278C006A0ABBA27DC8C63BF97F7E666E27C5284D7D3B1FFFE16B7A87B51D

     p=INTEGER:0xF3929B9435608F8A22C208D86795271D54EBDFB09DDEF539AB083DA912\
     D4BD57

     q=INTEGER:0xC50016F89DFF2561347ED1186A46E150E28BF2D0F539A1594BBD7FE467\
     46EC4F

     exp1=INTEGER:0x9E7D4326C924AFC1DEA40B45650134966D6F9DFA3A7F9D698CD4ABEA\
     9C0A39B9

     exp2=INTEGER:0xBA84003BB95355AFB7C50DF140C60513D0BA51D637272E355E397779\
     E7B2458F

     coeff=INTEGER:0x30B9E4F2AFA5AC679F920FC83F1F2DF1BAF1779CF989447FABC2F5\
     628657053A

This example is the corresponding public key in a SubjectPublicKeyInfo structure:

     # Start with a SEQUENCE
     asn1=SEQUENCE:pubkeyinfo

     # pubkeyinfo contains an algorithm identifier and the public key wrapped
     # in a BIT STRING
     [pubkeyinfo]
     algorithm=SEQUENCE:rsa_alg
     pubkey=BITWRAP,SEQUENCE:rsapubkey

     # algorithm ID for RSA is just an OID and a NULL
     [rsa_alg]
     algorithm=OID:rsaEncryption
     parameter=NULL

     # Actual public key: modulus and exponent
     [rsapubkey]
     n=INTEGER:0xBB6FE79432CC6EA2D8F970675A5A87BFBE1AFF0BE63E879F2AFFB93644\
     D4D2C6D000430DEC66ABF47829E74B8C5108623A1C0EE8BE217B3AD8D36D5EB4FCA1D9

     e=INTEGER:0x010001

# RETURN VALUES

`ASN1_generate_nconf()` and `ASN1_generate_v3()` return the encoded data as an ASN1_TYPE structure or NULL if an error occurred.

The error codes that can be obtained by ERR_get_error.

# SEE ALSO

ERR_get_error

# HISTORY

`ASN1_generate_nconf()` and `ASN1_generate_v3()` were added to OpenSSL 0.9.8