# Chamfer

[Chamfer] command chamfers specified curves

## Step 1

While "Specify 1st curve" prompt is displayed, click the mouse around an end point of the curve to chamfer

- Pressing the key`"D"`, a dialogue to input chamfer length will be shown.

- Pressing the key `"T"`, trim option will be changed. When this option is active, the part of curve from chamfer start point to end point wil be cut.

- Pressing the key `"J"`, joint option will be changed. When this option is active, the generated chamfer curve and the chamfered curve will be joined.

## Step 2

While "Specify 2nd curve" prompt is displayed, mouse-click on-curve point near an end point of another curve to chamfer.