Overview | Module | Use | Devguide | Index

Methods' Summary | Methods' Details | Attributes' Summary | Attributes' Details

:: com :: sun :: star :: awt ::
interface XSpinListener
  Base Hierarchy
      ::com::sun::star::uno::XInterface
       |
       +-::com::sun::star::lang::XEventListener
          |
          +-XSpinListener
Description makes it possible to receive spin events.

Methods' Summary
up | is invoked when the spin field is spun up.
down | is invoked when the spin field is spun down.
first | is invoked when the spin field is set to the lower value.
last | is invoked when the spin field is set to the upper value.

Methods' Details
up
[oneway] void up( | [in] SpinEvent | rEvent );
Description is invoked when the spin field is spun up.
down
[oneway] void down( | [in] SpinEvent | rEvent );
Description is invoked when the spin field is spun down.
first
[oneway] void first( | [in] SpinEvent | rEvent );
Description is invoked when the spin field is set to the lower value.
last
[oneway] void last( | [in] SpinEvent | rEvent );
Description is invoked when the spin field is set to the upper value.

Top of Page

Copyright © 2003 Sun Microsystems, Inc.