Overview | Module | Use | Devguide | Index

Elements' Summary | Elements' Details

:: com :: sun :: star :: ucb ::
struct RecipientInfo
Description contains all information needed to send a message using one send protocol. To send one message via two different protocols, two RecipientInfos are needed - to send one message to different users with one protocol, one RecipientInfo can be used.

Elements' Summary
ProtocolType | the protocol to use for sending (i.e. "NNTP", "SMTP", "VIM").
State | the current state of the message.
To | the recipient(s) (e.g. e-mail address/es).
CC | the recipient(s) of a "carbon copy" (e.g. e-mail address/es).
BCC | the recipient(s) of "blind carbon copy" (e.g. e-mail address/es).
Newsgroups | the newsgroup(s) to which an article is be posted.
Server | the name of the server to be used for sending the message.
Username | the user name to be used for authorizing on the send server.
Password | the password to be used for authorizing on the send server.
VIMPostOfficePath | the Post Office Path (VIM only).
ProtocolErrorString | string representing the last error (generated by send server).
ProtocolErrorNumber | the number representing the last error (generated by send server).
SendTries | the count of tries to send a message. This count is`1` if the message was sent with the first try and increases with every unsuccessful retry.

Elements' Details
ProtocolType
string ProtocolType; Description the protocol to use for sending (i.e. "NNTP", "SMTP", "VIM").
State
OutgoingMessageState State; Description the current state of the message.
To
string To; Description the recipient(s) (e.g. e-mail address/es). Multiple addresses are separated by commas.
CC
string CC; Description the recipient(s) of a "carbon copy" (e.g. e-mail address/es). Multiple addresses are separated by commas.
BCC
string BCC; Description the recipient(s) of "blind carbon copy" (e.g. e-mail address/es). Multiple addresses are separated by commas.
Newsgroups
string Newsgroups; Description the newsgroup(s) to which an article is be posted. Multiple addresses are separated by commas.
Server
string Server; Description the name of the server to be used for sending the message.
Username
string Username; Description the user name to be used for authorizing on the send server.
Password
string Password; Description the password to be used for authorizing on the send server.
VIMPostOfficePath
string VIMPostOfficePath; Description the Post Office Path (VIM only).
ProtocolErrorString
string ProtocolErrorString; Description string representing the last error (generated by send server).
ProtocolErrorNumber
long ProtocolErrorNumber; Description the number representing the last error (generated by send server).
SendTries
long SendTries; Description the count of tries to send a message. This count is`1` if the message was sent with the first try and increases with every unsuccessful retry.

Top of Page

Copyright © 2003 Sun Microsystems, Inc.