Overview | Namespace | Class | Index | Help

LIST OF: | VALUES

::

## enum RTParamMode

Summary
  specifies the mode of a parameter.
Description
  There are three paramter modes which have impact of the handling of the paramter in the UNO bridges and the UNO code generation.

#### Values
RT_PARAM_INVALID | Summary indicates an invalid parameter mode
RT_PARAM_IN | Summary indicates a pure in parameter which is used by value
RT_PARAM_OUT | Summary indicates a pure out parameter which is used by reference
RT_PARAM_INOUT | Summary indicates a in and out parameter which is used also by reference

Top of Page

Copyright © 2003 Sun Microsystems, Inc.