..
    **************************************************
    *                                                *
    *   Automatically generated file, do not edit!   *
    *                                                *
    **************************************************

.. _amdgpu_synid10_dst_mimg_gather4:

vdst
===========================

Image data to load by an *image_gather4* instruction.

*Size:* 4 data elements by default. Each data element occupies either 32 bits or 16 bits depending on :ref:`d16<amdgpu_synid_d16>`.

:ref:`d16<amdgpu_synid_d16>` and :ref:`tfe<amdgpu_synid_tfe>` affect operand size as follows:

* :ref:`d16<amdgpu_synid_d16>` specifies that data elements in registers are packed; each value occupies 16 bits.
* :ref:`tfe<amdgpu_synid_tfe>` adds one dword if specified.

*Operands:* :ref:`v<amdgpu_synid_v>`
