# mrcFFTMedianFilter

## Usage

    Usage: mrcFFTMedianFilter
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Essential :OutputDataFile
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-r                  r                   (1         )] :Optional  :Radius of Kernel Size (Pixel)
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----
    Calculation is performed on amplitude only.
    Output: Real part is amplitude and imaginary part is zero.
    Use this program only for CTF determination.