# ProjectionDirectionMapCreate

## Usage

    Usage: ProjectionDirectionMapCreate
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Optional  :OutputDataFile
        [-p[ost]s[cript]     Ps                  (NULL      )] :Optional  :OutputPostScriptFile
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
        [-R[otation]m[ode]   Rmode               (0         )] :Optional  :Mode
    ----- Rotational Mode -----
    Final rotation of projection is only Z .

    ----- input file format -----
    filename rotationalmode angle angle angle
       .             .        .     .     .
       .             .        .     .     .
       .             .        .     .     .
       .             .        .     .     .

    ----- mode -----
    -m : 0 : Not separate plus and minus of theta. Create one line data
         1 :     separate plus and minus of theta. Create one line data
         2 :     separate plus and minus of theta. Create two line data
         3 : Mollweide expressionn
    ----- mode -----
    -Rm : 0 : Not change rotational mode
          1 :     Change rotational mode to ZONS