# ctfWeightMapCreation

## Usage

    Usage: ctfWeightMapCreation
    Options:
        [-o[utput]           Out                 (stdout    )] :Optional  :OutputDataFile
        [-kV                 kV                  (200       )] :Optional  :AccVol[kV]
        [-Cs                 Cs                  (1.7       )] :Optional  :Cs[mm]
        [-df                 Defocus             (2.7       )] :Essential :Defocus[A]:under(+)
        [-white              WhiteNoise          (1.0       )] :Optional  :WhiteNoise(N/S)
        [-noise              Noise               (NULL      )] :Optional  :Noise Power Spectrum
        [-splusn             SplusN              (NULL      )] :Optional  :Signal+Noise Power Spectrum
        [-dRinv              dRinv               (1024*5/3  )] :Essential :dRinv[A]
        [-dRmaxInv           dRmaxInv            (10.0      )] :Essential :dRmaxInv[A]
        [-SinWin             SinWinRminInv       (20.0      )SinWinRmaxInv       (10.0      )] :Optional  :RminInv[A] RmaxInv[A]
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    Mode:
          0: No correction  : F = G
          1: Phase contrast : F = G*(H/abs(H))(Only 1 or -1)
          2: Phase contrast : F = G*H (Winer filter (S/N << 1))
          3: Phase contrast : F = G/H (Inverse filter)
          4: Phase contrast : F = G*(H/(H*H + N*N)) (Winer filter (white noise : Required Option -white))
          5: Phase contrast : F = G*(H/abs(H)*abs(G*G-N*N)/(G*G)) (Winer filter: Required Option -noise, -splusn))