MiMic Remote MCU

## About this page

Hello, This is MiMic Remote MCU. If you can see this page, MiMic RemoteMCU server is running.

## Onchip contents

- Setup
  This page setup webserver configulation.
- Local FileSystem
  Browse mbed Local FileSystem and SD card(only connected).
- JavaScript Editor
  MiMic JavaScript API test page. Here you can edit and test MiMicRemoteMCU via JavaScript API. JavaScript API is primary web interface to control MiMicRemoteMCU.
- MiMicIL Editor
  MiMicIL test page. Here you can edit and test the MiMicIL. MiMicIL is intermediate language is used to describe the byte code of MiMic.
- Memory Dump
  MCU Memory viewer. Display the contents of the memory of this MCU.

## Internet contents

- MiMic Website
  MiMic Website! There is information of MiMic.
- MiMic for Mbed repository
  MiMic for Mbed primary page. Source code here.
- JavascriptAPI reference
  MiMic Javascript API reference.
- MiMic project(SorceForge)
  MiMic for LPCXpresso and APIsfor other languages(PHP,Unit3D) . This is core library of MiMic.
- MiMic online samples(jsdo.it)
  Online sample programs using MiMic Javascript API.Those are tagged 'MiMic' programs at jsdo.it. jsdo.it is JavaScript sharing service.

## Reference

Software modules and development tool.

- MiMic SDK
  This is core module of MiMic.
- CodeMirror
  Onchip code editors are developed based on CodeMirror.
- uIP
  MiMicIP stack is created in reference to uIP 1.0.
- mbed.org
  MiMic for mbed can be compile by mbed online compiler.
- LPCXpresso NXPセミコンダクターズジャパン
  MiMic also works with LPCXpresso1768(1769).