## View and Operations

### Heatmap & 3D Display

#### 3D Display

##### 3D Display Settings

1. Select [Tools] in the menu bar and then select [Options] from the drop down menu.

2. Select [View] > [3D Display] in the Options dialog.

3. Enter the settings.

   Intensity Type:

   Relative

     The Z-axis in the 3D View is adjusted to the maximum intensity of the sample.

   Absolute

     You can specify the maximum intensity to be displayed on the Z-axis in the 3D View. Enter the value in the field below.

   Max Intensity:

   Enter a value when you select [Absolute] in [Intensity Type].

   Synchronized Rotation:

   Checking this box activates the synchronization of zoom and rotation of the 3D View of multiple samples.

   Draw Axis:

   Check this box if you want to display the scales on the axes of the 3D View.

4. Click [OK].