road:~#
 TESTNAME=nat-pluto-03
road:~#
 hostname road.uml.freeswan.org
road:~#
 ifconfig eth0 inet 192.1.3.194
road:~#
 route delete -net default 
SIOCDELRT: No such process
road:~#
 route add -net default gw 192.1.3.254
road:~#
 netstat -rn
Kernel IP routing table
Destination     Gateway         Genmask         Flags   MSS Window  irtt Iface
192.1.3.0       0.0.0.0         255.255.255.0   U         0 0          0 eth0
0.0.0.0         192.1.3.254     0.0.0.0         UG        0 0          0 eth0
road:~#
 source /testing/pluto/bin/roadlocal.sh
road:~#
 ipsec setup start
ipsec_setup: Starting Openswan IPsec VERSION
road:~#
 echo done
done
road:~#
 ipsec whack --name road-eastnet-forceencaps --initiate 
002 "road-eastnet-forceencaps" #1: initiating Main Mode
104 "road-eastnet-forceencaps" #1: STATE_MAIN_I1: initiate
003 "road-eastnet-forceencaps" #1: received Vendor ID payload [Openswan 
003 "road-eastnet-forceencaps" #1: received Vendor ID payload [Dead Peer Detection]
002 "road-eastnet-forceencaps" #1: transition from state STATE_MAIN_I1 to state STATE_MAIN_I2
106 "road-eastnet-forceencaps" #1: STATE_MAIN_I2: sent MI2, expecting MR2
002 "road-eastnet-forceencaps" #1: transition from state STATE_MAIN_I2 to state STATE_MAIN_I3
108 "road-eastnet-forceencaps" #1: STATE_MAIN_I3: sent MI3, expecting MR3
002 "road-eastnet-forceencaps" #1: Main mode peer ID is ID_FQDN: '@east'
002 "road-eastnet-forceencaps" #1: transition from state STATE_MAIN_I3 to state STATE_MAIN_I4
004 "road-eastnet-forceencaps" #1: STATE_MAIN_I4: ISAKMP SA established {auth=OAKLEY_RSA_SIG cipher=aes_128 prf=oakley_sha group=modp1536}
002 "road-eastnet-forceencaps" #2: initiating Quick Mode RSASIG+ENCRYPT+TUNNEL+PFS+UP+IKEv2ALLOW
117 "road-eastnet-forceencaps" #2: STATE_QUICK_I1: initiate
002 "road-eastnet-forceencaps" #2: transition from state STATE_QUICK_I1 to state STATE_QUICK_I2
004 "road-eastnet-forceencaps" #2: STATE_QUICK_I2: sent QI2, IPsec SA established tunnel mode
road:~#
 echo done.
done.
road:~#
 

road:~#
 ipsec setup stop
IPSEC EVENT: KLIPS device ipsec0 shut down.
ipsec_setup: Stopping Openswan IPsec...
road:~#
 kill `cat /var/run/klogd.pid`; cat /tmp/klog.log
klogd 1.3-3#33.1, log source = /proc/kmsg started.
road:~#
 halt -p -f
System halted.


