# $Id: sun3-carrera-eeprom.txt,v 1.1 2005/05/14 19:17:28 fredette Exp $

# sun3-carrera-eeprom.txt - input for tme-sun-eeprom to make an EEPROM
# image for Sun3 Carrera system:
#

# amount of memory installed and tested, in MB:
#
installed-#megs 8
selftest-#megs 0

# screen resolution:
#
screen-resolution 1152x900
screen-#columns 80
screen-#rows 34

# the console device:
#
console-device color-fb

# true if the watchdog causes a reset.
#
watchdog-reboot? false

# any boot device:
#
boot-device? true
boot-device sd(0,0,0)

# any OEM banner and/or logo bitmap.
#
oem-banner? false
oem-banner 
oem-logo? false
oem-logo 

# keyboard parameters.
#
keyboard-type sun
keyboard-locale 
keyboard-id 
keyboard-click? false

# the "diagnostic" boot device and file:
#
diag-device ie(0,0,0)
diag-file 

# inverse video (white-on-black, not implemented?)
#
inverse-video? false

# default parameters for ttya and ttyb:
#
ttya-mode 9600,8,n,1,-
ttyb-mode 9600,8,n,1,-

# security mode and password (only on PROM revisions > 2.7.0).
#
security-mode none
security-password 

# the 3/80 diagnostic "switch".
#
diag-switch? false

# "Factory Defined"
#
last-hardware-update 
