@c Copyright 2005
@c Free Software Foundation, Inc.
@c This is part of the GAS manual.
@c For copying conditions, see the file as.texinfo.
@ifset GENERIC
@page
@node M32C-Dependent
@chapter M32C Dependent Features
@end ifset
@ifclear GENERIC
@node Machine Dependencies
@chapter M32C Dependent Features
@end ifclear
 
@cindex M32C support

@code{@value{AS}} can assemble code for several different members of
the Renesas M32C family.  Normally the default is to assemble code for
the M16C microprocessor.  The @code{-m32c} option may be used to
change the default to the M32C microprocessor.

@menu
* M32C-Opts::                   M32C Options
@end menu
 
@node M32C-Opts
@section M32C Options
 
@cindex options, M32C
@cindex M32C options
 
The Renesas M32C version of @code{@value{AS}} has two
machine-dependent options:
 
@table @code
@item -m32c
@cindex @samp{-m32c} option, M32C
@cindex architecture options, M32C
@cindex M32C architecture option
Assemble M32C instructions.
 
@item -m16c
@cindex @samp{-m16c} option, M16C
@cindex architecture options, M16C
@cindex M16C architecture option
Assemble M16C instructions (default).
 
@end table
