MIPS Malta board

How to flash using a MIPS Navigator Probe:

  - Ensure that your Malta has jumper JP1 fitted. Without this jumper you will
    be unable to flash your Malta using a Navigator Probe.

  - Connect Navigator Console to your probe and Malta as usual.

  - Within Navigator Console run the following commands:

      source /path/to/u-boot/board/malta/flash-malta-boot.tcl
      reset
      flash-boot /path/to/u-boot/u-boot.bin

  - You should now be able to reboot your Malta to a U-boot shell.
