# Point from UV coordinates

[Point from UV coordinates] command displays point coordinates of surfaces, or generates points.

## Step 1

For the prompt "Specify a surface", select the target surface.

Pressing `C` key will change the mode between coordinates display mode and point generation mode.

## Step 2

For the prompt "Input parameters", input (u,v) parameters of the surface point from the dialogue.

After input, the command will evaluate the point, and generates the point as an object optionally.