# Parameter

This tab is used to set the facet parameters.

Curve tolerance

  Specifies tolerance used for boundary edges to approximate by polylines.

Max deviation

  Specifies tolerance used in surface facetting.

Maximum UV ratio

  Specifies the maximum aspect ratio of the (u,v) parameter space rectangles of the subdivided surfaces.

Max side length

  Specifies the maximum edge length of polygons to approximate the surface.

Minimum triangles

  Specifies the minimum number of triangles of the after-approximated polygons.

Remesh

  Update the preview of the polygon mesh.