# Tangent 4 edges command (Surface menu)

Use this command to make a surface from four curves that is tangent surfaces.

## Step 1

In the prompt Specify V-Min side curve, select a curve. This curve will be the V-Min perimeter of the surface to create.

## Step 2

In the prompt Select V-Min connecting surface, select surface(s). You may select zero, one, or multiple surfaces.

Press `Enter` to finish selection and go the next step.

## Step 3

In the prompt Specify U-Max side curve, select another curve. This curve will be the U-Max perimeter of the surface to create.

## Step 4

In the prompt Select U-Max connecting surface, select surfaces. You may select zero, one, or multiple surfaces.

Press `Enter` to finish selection and go the next step.

## Step 5

In the prompt Specify V-Max side curve, select another curve. This curve will be the V-Max perimeter of the surface to create.

## Step 6

In the prompt Select V-Max connecting surface, select surfaces. You may select zero, one, or multiple surfaces.

Press `Enter` to finish selection and go the next step.

## Step 7

In the prompt Specify U-Min side curve, select another curve. This curve will be the U-Min perimeter of the surface to create.

## Step 8

In the prompt Select U-Min connecting surface, select surfaces. You may select zero, one, or multiple surfaces.

Press `Enter` to finish selection and to generate the surface.