# UV Coordinates

UV Coordinates command evaluates UV coordinates of a surface point.

## Step 1

For the prompt "Select a surface to evaluate UV value", select a surface element.

The following options are provided:

- Pressing `C` key, the mode will be changed to the one that the point input will be generated as an object.

- Pressing `N` key, the command will show the (u,v) value by normalizing the coordinates to `[0, 1]` range.

## Step 2

For the prompt "Point to evaluate", select a point on the specified surface by mouse-click.