Overview | Module | Use | Devguide | Index

Methods' Summary | Methods' Details | Attributes' Summary | Attributes' Details

:: com :: sun :: star :: awt ::
interface XPrinterPropertySet
  Base Hierarchy
      ::com::sun::star::uno::XInterface
       |
       +-::com::sun::star::beans::XPropertySet
          |
          +-XPrinterPropertySet
Description represents an extended property set for printer properties. All properties are vetoable properties. If you change the properties between XPrinter::startPage and XPrinter::endPage , a ::com::sun::star::beans::PropertyVetoException is thrown. See also XPrinter See also XInfoPrinter

Methods' Summary
setHorizontal | sets the orientation.
getFormDescriptions | returns descriptions of all available printer forms.
selectForm | sets the form that should be used.
getBinarySetup | returns a binary encoded version of the printer setup.
setBinarySetup | sets the data specific to the printer driver.

Methods' Details
setHorizontal
void setHorizontal( | [in] boolean raises( | bHorizontal ) ::com::sun::star::beans::PropertyVetoException, ::com::sun::star::lang::IllegalArgumentException );
Description sets the orientation.
getFormDescriptions
sequence< string > getFormDescriptions(); |  |
Description returns descriptions of all available printer forms.
selectForm
void selectForm( | [in] string raises( | aFormDescription ) ::com::sun::star::beans::PropertyVetoException, ::com::sun::star::lang::IllegalArgumentException );
Description sets the form that should be used. Indirectly a printer is selected.
getBinarySetup
sequence< byte > getBinarySetup(); |  |
Description returns a binary encoded version of the printer setup.
setBinarySetup
void setBinarySetup( | [in] sequence< byte > raises( | data ) ::com::sun::star::beans::PropertyVetoException, ::com::sun::star::lang::IllegalArgumentException );
Description sets the data specific to the printer driver. Get this data from the info printer and set the data to the printer.

Top of Page

Copyright © 2003 Sun Microsystems, Inc.